OBVODY SE SBĚRNICÍ CAN

zdroj:http://can.marathon.ru

| Company | CAN Version | Microcontroller | Object Storage Capacity | Acceptance Filtering Capability | Bridge | Samples | Volume | Remarks | Website (Data Sheet and Application Notes)
T89C51CC01 | Atmel | 2.0B | 8-bit | 15 Tx/Rx buffers | 15 full-bit masks | no | now | n.a. | 256B RAM, 1KB ERAM, 32KB Flash, A/D, UART, TTCAN level 1 support, Autobaud, 40 MHz, TQFP44, PLCC44, CA-BGA64 | http://www.atmel-wm.com/
T89C51CC02 | Atmel | 2.0B | 8-bit | 4 Tx/Rx buffers | 4 full-bit masks | no | now | n.a. | 256B RAM, 256B ERAM, 16KB Flash, A/D, UART, TTCAN level 1 support, Autobaud, 40 MHz, PLCC28, SOIC28 | http://www.atmel-wm.com/
A_CAN | Bosch | 2.0B | none | 3 Tx / Rx buffers | 1 full-bit mask | no | n.a. | n.a. | Synthesizable IP module, CAN module with 3 configurable message buffers, flexible interface for 8-bit, 16-bit, or 32-bit CPU | http://www.can.bosch.com/
CAN Core | Bosch | 2.0B | none | n.a. | n. a. | no | n.a. | n.a. | Synthesizable IP module, CAN core cell with protocol controller and shift register | http://www.can.bosch.com/
CC750 | Bosch | 2.0B | none | 14 Tx/Rx buffers + 1 double Rx buffer | 2 global masks + 1 mask for Rx double buffer | no | now | now | function compatible with Intel 82527, interface to CPU by SPI only, SOIC16-W package | http://www.can.bosch.com/
CC770 | Bosch | 2.0B | none | 14 Tx/Rx buffers + 1 double Rx buffer | 2 global masks + 1 mask for Rx double buffer | no | now | now | pin and function compatible with Intel 82527, interface is 8/16-bit multiplexed/non-multiplexed | http://www.can.bosch.com/
C_CAN | Bosch | 2.0B | none | 32 Tx / Rx buffers | 32 full-bit masks | no | n.a. | n.a. | Synthesizable IP module, CAN module with message RAM for storage of 32 (or more) message objects, flexible interface for 8-bit, 16-bit, or 32-bit CPU | http://www.can.bosch.com/
TTCAN | Bosch | ISO11898–1,4 | none | 32 Tx / Rx buffers | 32 full-bit masks | no | n.a. | n.a. | Synthesizable IP module, CAN module with message RAM for storage of 32 message objects, flexible interface for 8-bit, or 16-bit CPU, TTCAN Level 2 support | http://www.can.bosch.com/
DS80C390 | Dallas | 2 x 2.0B | 8-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 14 Tx/Rx buffers + 1 double Rx buffer | possible | now | 1Q00 | 4kB SRAM, 256 x 16 RAM, 40 MHz clock rate, 16/32-bit math coprocessor | http://www.dalsemi.com/
MB90497G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 8 Tx/Rx buffers | 8 full-bit masks + 2 global masks | no | 2Q01 | 3Q01 | 64K Mask ROM, 2K RAM, UART, A/D, QFP64. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90548G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | 3Q02 | 1Q03 | 128KB Mask ROM, 4K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90549G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | now | 1Q01 | 256KB Mask ROM, 6K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90591 | Fujitsu | 2 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | n.a. | now | 384KB Mask ROM 8K RAM, UARTx3, A/D, 4 Stepper Motor Drivers, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90594 | Fujitsu | 2 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | n.a. | now | 256KB Mask ROM, 6K RAM, UARTx3, A/D, 4 Stepper Motor Drivers, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F387G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 8 Tx/Rx buffers | 8 full-bit masks + 2 global masks | no | 4Q01 | 1Q02 | 64K Flash, 2K RAM, UART, A/D, QFP48. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F428G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | now | 1Q01 | 128KB Flash, 6K RAM, UARTx2, A/D, 4 Stepper Motor Drivers, LCD, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F443G | Fujitsu | 3 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | 1Q01 | 2Q01 | 128KB Flash, 6K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F497G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 8 Tx/Rx buffers | 8 full-bit masks + 2 global masks | no | n.a. | now | 64K Flash, 2K RAM, UART, A/D, QFP64. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F543G | Fujitsu | 2 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | now | 1Q01 | 128KB Flash, 6K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F546G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | now | 1Q01 | 256KB Flash, 8K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F548G | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | 2Q01 | 3Q01 | 128KB Flash, 4K RAM, UARTx2, A/D, Ext Bus Interface, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F591 | Fujitsu | 2 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | n.a. | now | 384KB Flash 8K RAM, UARTx3, A/D, 4 Stepper Motor Drivers, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F594A | Fujitsu | 2 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | n.a. | now | 256KB Flash 6K RAM, UARTx3, A/D, 4 Stepper Motor Drivers, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB90F598 | Fujitsu | 1 x 2.0B | 16-bit (FFMC16LX) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | n.a. | now | 128KB Flash, 4K RAM, UARTx2, A/D, 4 Stepper Motor Drivers, QFP100. | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
MB91F361 | Fujitsu | 3 x 2.0B | 32-bit (FR) | 16 Tx / Rx buffers | 16 full-bit masks + 2 global masks | no | now | 4Q99 | 512KB Flash, 16K RAM, UARTx3, A/D, 4 Stepper Motor Drivers, 64MHz, LQFP208 | www.fujitsu-fme.com/index4.html?/products/micro/can/start.html
H8/300H | Hitachi | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | n.a. | n.a. | ASIC solution | semiconductor.hitachi.com/h8/?adjump=frontpage_products-section
H8S/2623 | Hitachi | 2.0B | 16-bit | 30 Tx/Rx buffers + 2 Rx buffers | 30 full-bit masks + 2 global masks | no | n.a. | n.a. | currently dedicated automotive customers only (open market support 3Q99 | semiconductor.hitachi.com/h8/?adjump=frontpage_products-section
SH7055 | Hitachi | 2.0B | 32-bit | 30 Tx/Rx buffers + 2 Rx buffers | 30 full-bit masks + 2 global masks | no | n.a. | n.a. |  | semiconductor.hitachi.com/superh/?adjump=frontpage_products-section
SuperH | Hitachi | 2.0B | 32-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | n.a. | n.a. | ASIC solution | semiconductor.hitachi.com/superh/?adjump=frontpage_products-section
C161CI | Infineon | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 256k ROM, 10k RAM, I2C, 2 x ASC, 2 x SSC, RTC | www.infineon.com/us/micro/can/content.html
C164CI | Infineon | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 64k OTP/ROM, 6 x PWM, RTC | www.infineon.com/us/micro/can/content.html
C167CR | Infineon | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | ROMless-, 32k or 128k ROM, 4xPWM | www.infineon.com/us/micro/can/content.html
C167CS | Infineon | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 11k RAM, ROMless, 32kROM, 4xPWM | www.infineon.com/us/micro/can/content.html
C505C/CA | Infineon | 2.0B | 8-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 32k OTP, ROM less, 16k or 32k ROM, 4 x PWM | www.infineon.com/us/micro/can/content.html
C515C | Infineon | 2.0B | 8-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 64k OTP, ROMless, 32k or 64k ROM, 4 x PWM | www.infineon.com/us/micro/can/content.html
SAE81C90/91 | Infineon | 2.0Bp | none | 16 Tx/Rx buffers | 16 full-bit masks | no | now | now | 2 x 8-bit I/O ports | www.infineon.com/us/micro/can/content.html
IniCAN | Inicore | 2.0B | 8-bit or DSP | implemenation-specific | implemention-specific | possible | n.a. | n.a. | technology independend functions for chip integrations | http://www.inicore.com/
AN82527 | Intel | 2.0B | none | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | developer.intel.com/design/auto/network.htm
AN87C196CA | Intel | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | developer.intel.com/design/auto/network.htm
AN87C196CB | Intel | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | developer.intel.com/design/auto/network.htm
AS82527 | Intel | 2.0B | none | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | developer.intel.com/design/auto/network.htm
AS87C196CB | Intel | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | developer.intel.com/design/auto/network.htm
MCP2510 | Microchip | 2.0B | none | 3 Tx buffers + 2 Rx buffers | 6 full-bit masks + 2 global masks | no | now | now | Stand-alone CAN Controller, SPI Interface, PDIP/SOIC18, TSSOP20 | http://www.microchip.com/
PIC18C658 | Microchip | 2.0B | 8-bit | 3 Tx buffers + 2 Rx buffers | 6 full-bit Acceptance Filters 2 Acceptance Masks | no | now | now | RISC MCU with 32K-byte Program Memory, 1.5K-bytes of SRAM, CAN 2.0B, 10bit-ADC, 9-bit Addressable USART, SPI, I2C,2xPWM's, in a 68L PLCC, 64L TQFP | http://www.microchip.com/
PIC18C858 | Microchip | 2.0B | 8-bit | 3 Tx buffers + 2 Rx buffers | 6 full-bit Acceptance Filters 2 Acceptance Masks | no | now | now | RISC MCU with 32K-byte Program Memory, 1.5K-bytes of SRAM, CAN 2.0B, 10bit-ADC, 9-bit Addressable USART, SPI, I2C, 2xPWM's, in a 80L TQFP, 84L PLCC | http://www.microchip.com/
CDC0806E | Micronas GmbH | 1 x 2.0B | 8-bit Flash | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | no | available | yes | 56k Byte Flash, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC0850E | Micronas GmbH | 1 x 2.0B | 8-bit MROM | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | no | available | yes | 56k Byte ROM, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC0860E | Micronas GmbH | 1 x 2.0B | 8-bit MROM | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | no | available | yes | 56k Byte ROM, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC1607F | Micronas GmbH | 3 x 2.0B | 16-bit Flash | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | yes | available | yes | 256k Byte Flash, 3 independent CAN-Modules, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC1630F | Micronas GmbH | 1 x 2.0B | 16-bit MROM | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | no | available | yes | 90k Byte ROM, 3 independent CAN-Modules, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC1650F | Micronas GmbH | 2 x 2.0B | 16-bit MROM | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | yes | available | yes | 128k Byte ROM, 3 independent CAN-Modules, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC1670F | Micronas GmbH | 2 x 2.0B | 16-bit MROM | 16 Tx/Rx buffers | 16 full-bit masks + 1 global mask | yes | available | yes | 216k Byte ROM, 3 independent CAN-Modules, 16 time-stamps | www.micronas.com/products/overview/automotive/index.php
CDC3207G | Micronas GmbH | 3 x 2.0B | 32-bit Flash | 32 Tx/Rx buffers per CAN | 32 full-bit masks + 1 global mask per CAN | yes | Q2/2001 | planned | 512k Byte Flash, 3 independent CAN-Modules, 32 time-stamps p. CAN | www.micronas.com/products/overview/automotive/index.php
CDC3210G | Micronas GmbH | 3 x 2.0B | 32-bit MROM | 32 Tx/Rx buffers per CAN | 32 full-bit masks + 1 global mask per CAN | yes | Q4/2001 | planned | 512k Byte ROM, 3 independent CAN-Modules, 32 time-stamps p. CAN | www.micronas.com/products/overview/automotive/index.php
CDC3230G | Micronas GmbH | 2 x 2.0B | 32-bit MROM | 32 Tx/Rx buffers per CAN | 32 full-bit masks + 1 global mask per CAN | yes | Q4/2001 | planned | 256k Byte ROM, 2 independent CAN-Modules, 32 time-stamps p. CAN | www.micronas.com/products/overview/automotive/index.php
CDC3250G | Micronas GmbH | 1 x 2.0B | 32-bit MROM | 32 Tx/Rx buffers | 32 full-bit masks + 1 global mask | no | Q4/2001 | planned | 128k Byte ROM, 1 independent CAN-Modules, 32 time-stamps | www.micronas.com/products/overview/automotive/index.php
M306NOMCT-xxxFP | Mitsubishi | 2 x 2.0B | 16-bit | 16 Tx/Rx buffers | 16 full-bit masks + 3 global masks | yes | now | now | 2 independent on-chip CAN modules, 3 phase motor controllers | http://www.mitsubishichips.com/
M37630M4-xxxFP | Mitsubishi | 2.0B | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 full-bit mask + 1 global mask | no | now | now |  | http://www.mitsubishichips.com/
M37632MF-xxxFP | Mitsubishi | 2.0B | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 full-bit mask + 1 global mask | no | now | now |  | http://www.mitsubishichips.com/
68HC(7)05X32 | Motorola | 2.0A | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 global 8-bit mask | no | now | now | 64-pin packaging (32K ROM) | mcu.motsps.com/documentation/
68HC05X16 | Motorola | 2.0A | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 global 8-bit mask | no | now | now | 64-pin packaging (16K ROM) | mcu.motsps.com/documentation/
68HC(7)05X4 | Motorola | 2.0A | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 global 8-bit mask | no | now | now | 28-pin packaging (4K ROM) | mcu.motsps.com/documentation/
68HC908AZ60A | Motorola | 2.0B | 8-bit | 3 Tx buffers + 2 Rx buffers | 1 global 32-bit or 2 global 16-bit or 4 global 8-bit masks | no | Feb 01 | Apr 01 | 64-pin packaging (60K flash) | mcu.motsps.com/documentation/
68HC08AZ60 | Motorola | 2.0B | 8-bit | 3 Tx buffers + 2 Rx buffers | 1 global 32-bit or 2 global 16-bit or 4 global 8-bit masks | no | now | now | 64-pin packaging (60K ROM) | mcu.motsps.com/documentation/
68HC08AZ32A | Motorola | 2.0B | 8-bit | 3 Tx buffers + 2 Rx buffers | 1 global 32-bit or 2 global 16-bit or 4 global 8-bit masks | no | Mrz 01 | Jun 01 | 64-pin packaging (32K ROM) | mcu.motsps.com/documentation/
68HC912BC32 | Motorola | 2.0B | 16-bit | 3 Tx buffers + 2 Rx buffers | 1 global 32-bit or 2 global 16-bit or 4 global 8-bit masks | no | now | now | 80-pin packaging (32K flash) | mcu.motsps.com/documentation/
68HC912D60 | Motorola | 2.0B | 16-bit | 3 Tx buffers + 2 Rx buffers | 1 global 32-bit or 2 global 16-bit or 4 global 8-bit masks | no | now | now | 80-pin or 112-pin packaging (60K flash) | mcu.motsps.com/documentation/
68HC912DG128 | Motorola | 2 x 2.0B | 16-bit | 3 Tx buffers + 2 Rx buffers | 2 global 32-bit or 4 global 16-bit or 8 global 8-bit masks | yes | now | now | 2 independent on-chip CAN modules, 112-pin packaging (128K flash) | mcu.motsps.com/documentation/
68HC912DT128A | Motorola | 3 x 2.0B | 16-bit | 3 Tx buffers + 2 Rx buffers | 2 global 32-bit or 4 global 16-bit or 8 global 8-bit masks | yes | now | now | 3 independent on-chip CAN modules, 112-pin packaging (128K flash) | mcu.motsps.com/documentation/
MC9S12DP256 | Motorola | 5 x 2.0B | 16-bit | 3 Tx buffers + 4 Rx buffers | 2 global 32-bit or 4 global 16-bit or 8 global 8-bit masks | yes | now | Q102 | 5 independent on-chip CAN modules, 80-pin or 112-pin packaging (128K flash) | mcu.motsps.com/documentation/
MC68F375 (CERBERUS) | Motorola | 2.0B | 32-bit | 16 Tx/Rx buffers | 16 full-bit masks + 3 global masks | no | now | now | time-stamp, 256K flash memory | mcu.motsps.com/documentation/
MC68376 | Motorola | 2.0B | 32-bit | 16 Tx/Rx buffers | 16 full-bit masks + 3 global masks | no | now | now | time-stamp | mcu.motsps.com/documentation/
MC68377 (EXCALIBUR) | Motorola | 2.0B | 32-bit | 16 Tx/Rx buffers | 16 full-bit masks + 3 global masks | no | now | now | time-stamp | mcu.motsps.com/documentation/
MPC555 (BLACK OAK) | Motorola | 2 x 2.0B | 32-bit | 32 Tx/Rx buffers | 32 full-bit masks + 6 global masks | yes | now | 4Q99 | 2 independent on-chip CAN modules, time-stamp, 448K flash memory | mcu.motsps.com/documentation/
MPC565 (SPANISH OAK) | Motorola | 3 x 2.0B | 32-bit | 48 Tx/Rx buffers | 48 full-bit masks + 9 global masks | yes | LIMITED | 4Q01 | 3 independent on-chip CAN modules, time-stamp, 1M flash memory | mcu.motsps.com/documentation/
COP684BC | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | www.national.com/search/search.cgi/main?keywords=COP684BC
COP688/89EB | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | www.national.com/search/search.cgi/main?keywords=COP688
COP87/L88/89EB | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | http://www.national.com/search/search.cgi/main?keywords=COP688
COP87L84BC | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | www.national.com/search/search.cgi/main?keywords=COP87
COP888/89EB | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | www.national.com/search/search.cgi/main?keywords=COP888
COP8884BC | NatSem | 2.0Bp | 8-bit | 1 Tx 2-byte buffer + 2 Rx 2-byte buffers | 1 global 8-bit mask | no | now | now | 8-byte frames can be handles up to 125 kbit/s | www.national.com/search/search.cgi/main?keywords=COP888
CR16MCS9VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Flash memory, Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MCS9VE
CR16MAS9VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Flash memory, Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MAS9VJE
CR16MAS5VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MAS5VJE
CR16MBR5VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MBR5VJE
CR16MAS5VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MAS5VJE
CR16MCS5VJE | NatSem | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 14 full-bit masks + 1 global mask | no | now | now | Extended Temperature Range | www.national.com/search/search.cgi/main?keywords=CR16MCS5VJE
ATOMIC - D703121 | NEC | 2 x 2.0B | 32-bit RISC | 32 Tx/Rx buffers | 32 full-bit masks + 3'4 29-bit masks | possible | 4Q00 | 1Q01 | 128k Flash, QFP144, LCD, CAN Time System, 2x FCAN | http://www.nec.de/
ATOMIC - D703123 | NEC | 3 x 2.0B | 32-bit RISC | 64 Tx/Rx buffers | 64 full-bit masks + 3'4 29-bit masks | possible | 1Q00 | 3Q00 | 256k Flash, QFP144, LCD, CAN Time System, 3x FCAN | http://www.nec.de/
ATOMIC - µPD703121 | NEC | 2 x 2.0B | 32-bit RISC (V850E) | 32 Tx/Rx buffers | 32 full-bit masks + 4 global 29-bit masks | possible | 4Q00 | 1Q01 | 128k Flash, QFP144, LCD, CAN Time System, 2x FCAN | http://www.nec.de/
ATOMIC - µPD703123 | NEC | 3 x 2.0B | 32-bit RISC (V850E) | 64 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | possible | 1Q00 | 3Q00 | 256k Flash, QFP144, LCD, CAN Time System, 3x FCAN | http://www.nec.de/
ATOMIC - µPD70F3123 | NEC | 3 x 2.0B | 32-bit RISC (V850E) | 64 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | possible | 4Q99 | 3Q00 | 256k Flash, QFP144, LCD, CAN Time System, 3x FCAN | http://www.nec.de/
CANASSP1 - µPD780948 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | now | 60k, QFP100, LCD, CAN Time System | http://www.nec.de/
CANASSP1 - µPD780949 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | 2Q00 | D780948 + EEPROM | http://www.nec.de/
CANASSP1 - µPD78F0948 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | now | 60k Flash, QFP100, LCD, CAN Time System | http://www.nec.de/
CANASSP1 - µPD78F0949 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | 2Q00 | D78F0948 + EEPROM | http://www.nec.de/
CANASSP2 - µPD 78F0818 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | 3Q00 | D78081X with 60k Flash | http://www.nec.de/
CANASSP2 - µPD780814/6 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | 1Q00 | 4Q00 | 32/48k, QFP64, EEPROM, CAN Time System | http://www.nec.de/
CANASSP3 - µPD 78F0828 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | now | 2Q00 | D78082X with 60k Flash | http://www.nec.de/
CANASSP3 - µPD780824/6 | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | 3Q99 | 1Q00 | 32/48k, QFP80, LCD, EEPROM, Stepper motor driver, CAN Time System | http://www.nec.de/
MiniCAN - µPD789850 | NEC | 2.0B | 8-bit (78K0S) | 2 Tx buffers + 14 Rx buffers | 14 full-bit masks + 2 global 29-bit masks | no | 1Q00 | 4Q00 | 16k, SSOP30, CAN Time System | http://www.nec.de/
MiniCAN - µPD78F9850 | NEC | 2.0B | 8-bit (78K0S) | 2 Tx buffers + 14 Rx buffers | 14 full-bit masks + 2 global 29-bit masks | no | 1Q00 | 4Q00 | 16k Flash, SSOP30, CAN Time System | http://www.nec.de/
PHOENIX - µPD703116 | NEC | 2.0B | 32-bit RISC (V850E) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | Jun 00 | Apr 01 | 128k Mask-ROM, 6kRAM, 7x16-bit timers (inverter control PWM output); FCAN, 2xCSI, 3xUART, 2 x 8ch x 10bit AD, 144pin QFP | http://www.nec.de/
PHOENIX - µPD70F3116 | NEC | 2.0B | 32-bit RISC (V850E) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | Dez 99 | n.a. | 256kFlash, 10kRAM, 7x16-bit timers (inverter control PWM output); FCAN, 2xCSI, 3xUART, 2 x 8ch x 10bit AD, 144pin QFP | http://www.nec.de/
SCAN - µPD703076Y | NEC | 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | n.a. | Jan 01 | 128k Mask-ROM, 10kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
SCAN - µPD703077Y | NEC | 2 x 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | n.a. | Jan 01 | 256k Mask-ROM, 10kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
SCAN - µPD703078Y | NEC | 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | n.a. | Okt 01 | 256k Mask-ROM, 16kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
SCAN - µPD703079Y | NEC | 2 x 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | n.a. | Okt 01 | 256k Mask-ROM, 16kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
SCAN - µPD70F3077Y | NEC | 2 x 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | Apr 01 | Dez 01 | 128kFlash, 10kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
SCAN - µPD70F3079Y | NEC | 2 x 2.0B | 32-bit RISC (V850) | 32 Tx/Rx buffers | 64 full-bit masks + 4 global 29-bit masks | no | Jan 00 | Aug 00 | 256kFlash, 16kRAM, 8x16-bit timers; 2xFCAN, 4xCSI, 2xUART, 1 x I2C, 12ch x 10bit AD, POR, 100pin QFP | http://www.nec.de/
µPD780701Y | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | n.a. | 11/00 | 60k Mask-ROM, 3k RAM, 16 x 8-bit A/D, 7 timers, IE-Bus controller, 3 x 8-bit PWM-outputs, 4 serial I/O, 80 pin QFP | http://www.nec.de/
µPD78F0701Y | NEC | 2.0B | 8-bit (78K0) | 2 Tx buffers + 16 Rx buffers | 16 full-bit masks + 2 global 29-bit masks | no | 4/00 | tbd | 60k Flash, 3k RAM, 16 x 8-bit A/D, 7 timers, IE-Bus controller, 3 x 8-bit PWM-outputs, 4 serial I/O, 80 pin QFP | http://www.nec.de/
MSM9225 | OKI Electric | 2.0B | none | 16 Tx/Rx buffers | 16 full-bit masks | no | now | now |  | http://www.oki-europe.de/
P82C150 | Philips | 2.0Bp | SLIO | n.a. | n. a. | no | now | now | in maintenance state, not for new desing-ins | www-us.semiconductors.philips.com/can/products/
P8XC591 | Philips | 2.0B | 8-bit | 1 Tx buffer + 64 Rx FIFO | 1 global 32-bit mask or 2 global 16-bit masks | no | now | 1Q00 |  | www-us.semiconductors.philips.com/can/products/
P8XC592/8 | Philips | 2.0A | 8-bit | 1 Tx buffer + 2 Rx buffers | 1 global 8-bit mask | no | now | now |  | www-us.semiconductors.philips.com/can/products/
P8XC59X | Philips | 2.0B | 8-bit | to be defined | to be defined | no | 2Q00 | 3Q00 | will replace P8x592/8 | www-us.semiconductors.philips.com/can/products/
SJA1000 | Philips | 2.0B | none | 1 Tx buffer + 64 Rx FIFO | 1 global 32-bit mask or 2 global 16-bit masks | no | now | now | replaces 82C200 | www-us.semiconductors.philips.com/can/products/
XA-C3 | Philips | 2.0B | 16-bit | 32 Tx/Rx buffers | 32 full-bit masks + global masks | no | 4Q99 | 1Q00 | CANopen, DeviceNet and OSEK transport layer hardwired | www-us.semiconductors.philips.com/can/products/
CAN Core | Sican | 2.0B | optional | implementation-specific | implementation-specific | possible | now | now | CAN Core, VHDL- and Verilog Model for ASIC and FPGA | http://www.sican.com/
L9942/ST6 | ST-Microelectronics | 2.0A | 8-bit | 1 Tx buffer + 1 Rx buffer | 1 global 11-bit mask | no | now | 4Q99 | 40V SuperSmartPower, OTP, ROM versions (2Q00) | mcu.st.com
ST10F1167 | ST-Microelectronics | 2.0B | 16-bit | 14 Tx/Rx buffers + 1 double Rx buffer | 14 Tx/Rx buffers + 1 double Rx buffer | no | now | now | 128 kbyte flash, 32k or ROMless | mcu.st.com
ST72511R4 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | now (ROM 1Q00) | 16k, TQFP64 | mcu.st.com
ST72511R6 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | now (ROM 1Q00) | 32k, TQFP64 | mcu.st.com
ST72511R7 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | now (ROM 1Q00) | 48k, TQFP64 | mcu.st.com
ST72511R9 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | now (ROM 1Q00) | 60k, TQFP64 | mcu.st.com
ST72532J4 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | 1Q00 | 2Q00 (ROM 3Q00) | 16k, 256EE, TQFP44 | mcu.st.com
ST72532K4 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | 1Q00 | 2Q00 (ROM 3Q00) | 16k, 256EE, SO34 | mcu.st.com
ST72532R4 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | now (ROM 3Q00) | 16k, 256EE, TQFP64 | mcu.st.com
UD05 | ST-Microelectronics | 2.0Bp | 8-bit | 3 Tx/Rx buffers | 2 global 11-bit masks | no | now | 4Q99 | 40V SuperSmartPower, OTP, ROM versions (2Q00) | mcu.st.com
TMS320LF2406 | Texas Instruments | 2.0B | 16-bit DSP | 6 Tx/Rx buffers | 2 full-bit masks + 1 global mask | no | now | now | 32k x 16 flash, 2.5k x 16 RAM, 16 x 10-bit A/D, 16 x PWM, QEP, SCI, SPI | http://www.ti.com/
TMS320LF2407 | Texas Instruments | 2.0B | 16-bit DSP | 6 Tx/Rx buffers | 2 full-bit masks + 1 global mask | no | now | now | 32k x 16 flash, 2.5k x 16 RAM, 16 x 10-bit A/D, 16 x PWM, QEP, SCI, SPI | http://www.ti.com/
TMS320LC2406 | Texas Instruments | 2.0B | 16-bit DSP | 6 Tx/Rx buffers | 2 full-bit masks + 1 global mask | no | now | now | 2.5k x 16 RAM, 16 x 10-bit A/D, 16 x PWM, QEP, SCI, SPI | http://www.ti.com/
TMS320F241 | Texas Instruments | 2.0B | 16-bit DSP | 6 Tx/Rx buffers | 2 full-bit masks + 1 global mask | no | now | now | 8k x 16 flash, 544 x 16 RAM, 8 x 10-bit A/D, 8 x PWM, QEP, SCI, SPI | http://www.ti.com/
TMS320F243 | Texas Instruments | 2.0B | 16-bit DSP | 6 Tx/Rx buffers | 2 full-bit masks + 1 global mask | no | now | now | 8k x 16 flash, 544 x 16 RAM, 8 x 10-bit A/D, 8 x PWM, QEP, SCI, SPI | http://www.ti.com/
TC190C580 | Toshiba | 2.0B | none | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now |  | http://doc.semicon.toshiba.co.jp/
TMP86CH87U | Toshiba | 2.0B | 16-bit | 7 Tx/Rx buffers + 1 Rx buffer | 7 full-bit masks + 1 global mask | no | Q3/01 | Q4/01 | 16kB Mask ROM | http://doc.semicon.toshiba.co.jp/
TMP86PH87U | Toshiba | 2.0B | 16-bit | 7 Tx/Rx buffers + 1 Rx buffer | 7 full-bit masks + 1 global mask | no | Q2/01 | Q3/01 | 16kB OTP ROM | http://doc.semicon.toshiba.co.jp/
TMP91CM80F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 32kB Mask ROM | http://doc.semicon.toshiba.co.jp/
TMP91PP80F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 48kB OTP ROM | http://doc.semicon.toshiba.co.jp/
TMP95CS54F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 64kB Mask ROM | http://doc.semicon.toshiba.co.jp/
TMP95CU54F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 96kB Mask ROM | http://doc.semicon.toshiba.co.jp/
TMP95PS54F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 64kB OTP ROM | http://doc.semicon.toshiba.co.jp/
TMP95FW54F | Toshiba | 2.0B | 16-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | now | now | 128kB Flash | http://doc.semicon.toshiba.co.jp/
TMP92CW53F | Toshiba | 2.0B | 32-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | Q2/01 | Q3/01 | 128kB Mask ROM | http://doc.semicon.toshiba.co.jp/
TMP94FY53F | Toshiba | 2.0B | 32-bit | 15 Tx/Rx buffers + 1 Rx buffer | 15 full-bit masks + 1 global mask | no | Q2/01 | Q3/01 | 256kB Flash ROM | http://doc.semicon.toshiba.co.jp/
TMPR3903BF | Toshiba | 2.0B | 32-bit | 30 Tx/Rx buffers + 2 Rx buffer | 30 full-bit masks + 2 global mask | no | Q1/02 | Q2/02 | analog graphics ctr. for driver information / telematic systems | http://doc.semicon.toshiba.co.jp/